**PUBLIC NOTICE OF COPPER RETIREMENT UNDER RULE 51.333**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Network Disclosure Number:** | | | **ATT20230016C.1** | Issue Date: | **2/23/2023** |
|  | |  | | | |
| **Carrier’s Name:** | Michigan Bell Telephone Company d/b/a AT&T Michigan | | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Carrier’s Address:** | | 1120 20th Street NW, Suite 1000, Washington, DC 20036 | |  | |
| **Contact:** | Your Account Manager or Service Representative  For Technical Issues: | | | |
|  | Mark Peters | | Wendy Scott | |
| 1116 Houston St, Rm 738 | | 211 S Akard St, 11th Floor | |
| Fort Worth, TX 76102 | | Dallas, TX 75202 | |
| 972-706-7633 | | 714-925-4704 | |
| [mp2586@att.com](mailto:mp2586@att.com) | | [ws6715@att.com](mailto:ws6715@att.com) | |

**Implementation Date:** On or after June 23, 2023

**Description of Network Changes Planned:**

Michigan Bell Telephone Company d/b/a AT&T Michigan intends to retire copper facilities serving distribution area (DA) 4209 in the Kalamazoo wire center (KLMZMIFA) due to the impact of a jointly planned city of Kalamazoo and Michigan Department of Transportation (MDOT) road improvement project. This road construction will replace the Inkster Avenue bridge over Bronson Boulevard in Kalamazoo, Michigan. The city and MDOT have requested AT&T Michigan to remove or relocate its facilities in the way of the road project before June 30, 2023.

AT&T Michigan plans to migrate the customers served by copper facilities to existing Gigabit Passive Optical Network/Fiber-to-the-Premises (GPON/FTTP) facilities, and then retire the copper facilities.

**Description of Reasonably Foreseeable Impact of the Planned Changes:**

After implementation of this plan, services requiring copper facilities will no longer be available in this DA. Currently, AT&T Michigan records indicate a total of 30 assigned circuits, one of which is a competitive carrier circuit. Notice has been sent to the affected carrier to make alternative arrangements.

**Impacted addresses:**

****