**PUBLIC NOTICE OF COPPER RETIREMENT UNDER RULE 51.333**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Network Disclosure Number:** | | | **ATT20250010C.1** | Issue Date: | **1/16/2025** |
|  | |  | | | |
| **Carrier’s Name:** | BellSouth Telecommunications, LLC d/b/a AT&T Tennessee | | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Carrier’s Address:** | | 601 New Jersey Avenue NW, 5th FL, Washington, DC 20001 | |  | |
| **Contact:** | Your Account Manager or Service Representative  For Technical Issues: | | | |
|  | Mark Peters | | Wendy Scott | |
| 211 S. Akard St, 11th Floor | | 211 S Akard St, 11th Floor | |
| Dallas, TX 75202 | | Dallas, TX 75202 | |
| 972-706-7633 | | 714-925-4704 | |
| [mp2586@att.com](mailto:mp2586@att.com) | | [ws6715@att.com](mailto:ws6715@att.com) | |

**Implementation Date:** On or after May 16, 2025

**Description of Network Changes Planned:**

BellSouth Telecommunications, LLC d/b/a AT&T Tennessee intends to retire copper facilities serving distribution areas (DA) 3301, 3310, and 3326 in the Murfreesboro wire center (MRBOTNMA) due to the impact of a City of Murfreesboro and Tennessee Department of Transportation (TDOT) jointly planned road construction project. This project will widen Bradyville Pike from SE Broad Street to Rutherford Boulevard. The city and TDOT have requested AT&T Tennessee to remove or relocate its facilities in the way of this project before June 30, 2025.

AT&T Tennessee plans to migrate customers currently served by copper facilities to existing Gigabit Passive Optical Network/Fiber-to-the-Premises (GPON/FTTP) facilities and then retire the copper facilities.

**Description of Reasonably Foreseeable Impact of the Planned Changes:**

After implementation of this plan, only fiber-based services will be available to serve these DAs. Currently, AT&T Tennessee records indicate a total of 20 assigned circuits, none of which are competitive carrier circuits, affected by this network change.

**Attachment of Impacted Addresses:**

****