Centrex Resale Service

This composite shows the relative location of the fields from this practice in the transaction set.  An actual transaction would also contain required fields from the LSR and End User practices.

ST~850~0001

BEG…

{CENTREX Common Block}

PO1~1~1~EA~~~A6~CTXCB        
SI~TI~CB~CB
{One SLN per Station Number}
SLN~1~1~A                                    

SI~TI~SA~SNA

SI~TI~PX~SN
{CENTREX Station Details}

PO1~2~1~EA~~~A6~CTXSD         
SI~TI~NQ~NPI
SI~TI~SA~LNA
SI~TI~LO~LST

SI~TI~TN~TNS
SI~TI~T5~TERS
SI~TI~CN~ECCKT
SI~TI~OT~OTN
SI~TI~SN~ISPID

SI~TI~IK~ISDNP
SI~TI~T3~JK CODE
SI~TI~T7~JK NUM
SI~TI~T1~JK POS
SI~TI~T6~TCOPT

SI~TI~SY~SSIG

PID~X~~TI~CFA~CFA
PID~S~~TI~AG~~~SO-RSQ~NIDR
PID~S~~TI~AM~~~SO-RSQ~JR
PID~S~~AS~SAI~~~ATT01~SAI
REF~IX~LNUM~LNUM

REF~GP~TSP
DTM~376~TC PER

N9~H7~LOC~AAI

MTX~~AAI

N1~IT~NAME
N4~~STATE~ZIP
NX2~07~CITY
NX2~59~SAPR
NX2~01~SANO
NX2~61~SASF
NX2~03~SASD
NX2~02~SASN (1-55)
NX2~15~SASN (56-60)
NX2~62~SATH
NX2~40~SASS
See Conversion Tables for LDn/LVn conversion/mapping information

NX2~{LD1}~LV1
NX2~{LD2}~LV2
NX2~{LD3}~LV3
PER~CA~LCON~TE~TEL NO

SI~TI~AF~AFT

SI~TI~NW~NCON
N1~8V~~41~LPIC
N1~P9~~41~PIC
{one SLN loop per BA/BLOCKING pair}

SLN~2~1~A

SI~TI~BB~BA

SI~TI~TB~BLOCK
{one SLN per IWJK/IWJQ pair}

SLN~2~2~A~IWJQ~EA~~~~EQ~IWJK
SLN~2~3~A

SI~TI~TC~TC TO PRI
N1~TT~TC NAME
REF~55~TCID~PRI

SLN~2~4~A

SI~TI~TC~TC TO SEC
N1~TT~TC NAME
REF~55~TCID~SEC

{one SLN loop per FEATURE}

SLN~2~5~A              
SI~TI~SA~FA

SI~TI~SF/SC~FEATURE

SI~TI~FD~FEATURE DETAIL (1-48)~99~FEATURE DETAIL (49-96)~99~FEATURE DETAIL (97-144)~99~FEATURE DETAIL (145-192)~99~FEATURE DETAIL (193-200)
CTT~{# of PO1}

SE~{# of segments}~0001
